**Bulldogs Racing** [213]

**Fuse Table**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Fuse ID** | **Part** | **Continuous Conductor Rating** (A) | **Max Voltage** (V) | **Rating** (A) | **Interrupt Rating** |
| Pump | Littelfuse ATOF Blade Fuse | 10 | 12 | 3 | 1kA @ 32V |
| Motor Controller Left | Littelfuse ATOF Blade Fuse | 7 | 12 | 2 | 1kA @ 32V |
| Motor Controller Right | Littelfuse ATOF Blade Fuse | 7 | 12 | 3 | 1kA @ 32V |
| Beaglebone | Littelfuse ATOF Blade Fuse | 5 | 12 | 2 | 1kA @ 32V |
| HV Control | Littelfuse ATOF Blade Fuse | 7 | 12 | 3 | 1kA @ 32V |
| AMS | Littelfuse ATOF Blade Fuse | 7 | 12 | 2 | 1kA @ 32V |
| IMD | Littelfuse ATOF Blade Fuse | 7 | 12 | 2 | 1kA @ 32V |
| Energy Meter | Littelfuse ATOF Blade Fuse | 7 | 12 | 2 | 1kA @ 32V |
| Transponder | Littelfuse ATOF Blade Fuse | 5 | 12 | 2 | 1kA @ 32V |
| Brake Light | Littelfuse ATOF Blade Fuse | 5 | 12 | 2 | 1kA @ 32V |
| Charge Gauge | Littelfuse ATOF Blade Fuse | 7 | 12 | 2 | 1kA @ 32V |
| Speedometer | Littelfuse ATOF Blade Fuse | 7 | 12 | 2 | 1kA @ 32V |
| Master LV | Littelfuse ATOF Blade Fuse | 10 | 14 | 7.5 | 1kA @ 32V |
| Charging | Littelfuse 0487010.MXP | 10 | 300 | 10 | 300A @ 420V |
| *Holder* | MPD BF303 | - | - | 10 | - |
| HV Lighting | Littelfuse ATOF Blade Fuse | 5 | 12 | 1 | 1kA @ 32V |
| *Holder* | MPD BK-6010 | - | - | 30 | - |
| AMS Test (x4) | Schurter 0001.2504 | 7 | 300 | 1 | 5000 – 1000 A |
| *Holder* | MPD BF303 | - | - | 10 | - |
| Main Tractive System | Littelfuse L50S225 | 260 | 300 | 225 | 20 kA |